It is recommended that bolts remain “hand tight” until all bolts are installed.

Package includes:

|  |  |
| --- | --- |
| Roof Panel | Rear Dust Panel |
| Dust Covers | Dust Cover Clips |
| * 16-  ¼-20 x ¾” button head (black)
* 16-  ¼” flat washer (black)
* 9-    ¼´ flanged nylock nut (zinc)

Bolt Kit |

|  |  |
| --- | --- |
| STEP 1 | * Mount the Rear Dust Panel using the provided bolts.
 |
| STEP 2 | * Set the individual Dust covers in place.

Note: this view is from the driver seat looking up. |
| STEP3 | * Secure each dust cover using the provided bolts with flat washers and the Dust Cover Clips.

Note: Light bar is not included in the package. |

|  |  |
| --- | --- |
| STEP 4 | * Secure the four rear bolts by aligning the holes with corresponding holes of the Rear Dust panel and inserting the provided bolts with flat washers.
 |
| STEP 5 | * Secure the front by aligning the three holes in the Roof Panel with the corresponding holes in the machines front roll cage panel, indicated in this illustration
 |
| STEP 6 | * Tighten all bolts.
 |