**Safety:**

* Ensure that the UTV is safely parked on level ground with the ignition off.
* Wear all appropriate PPE for the following procedures.

**Note:**

* Leave all hardware loose until the entire assembly is in its final position.

**Assembly Components:**

Ensure that you have all of these components before beginning the installation.

**1 x Bumper**

**2 x Lower Mounting Brackets (left and right)**

**2 x Upper Mounting Brackets (left and right)**

**1 x Aluminum Accent Plate**

**1 x Hardware Kit**


****

Figure 1: Kit Contents

**Installation:**

1. Attach the aluminum accent plate to the inside of the bumper using the 2 small machine screws and nuts.



Figure 2: Accent Plate Front

1. Attach the left and right lower mounting brackets to the bumper using 4 short carriage bolts and nuts.

****

Figure 3: Upper Brackets to Bumper

1. Remove the factory bolts below the tailgate to allow for future installation of the upper mounting brackets. Shown in Figure 4.

****

Figure 4: Factory Bolts for Removal

1. Position the lower mounting brackets with the mounting location shown in Figure 5, and secure them using 4 long carriage bolts and nuts.


****

Figure 5: Lower Bracket Mounting Location


****

Figure 6: Lower Brackets to Machine

1. Align the left and right upper mounting brackets with the mounting location on the bumper and machine and secure using short bolts.

****

Figure 7: Upper Bracket to Machine and Bumper

1. Tighten all hardware securely, and enjoy your ride!



Figure 8: Install Complete