**Safety:**

* Ensure that the UTV is safely parked on level ground with the ignition off.
* Wear all appropriate PPE for the following procedures.

**Note:**

* Leave all hardware loose until the entire assembly is in its final position.

**Assembly Components:**

Ensure that you have all of these components before beginning the installation.

**1 x Windshield**

**1 x Trimlock Seal**

**8 x 1.7” Roll Bar Clamps**

**1 x Windshield Wiper**

**1 x Wiper Lever**

**1 x Hardware Kit**

****

Figure : Windshield Kit Contents

**Windshield Installation:**

1. Install the Trimlock seal onto the bottom edge of the windshield. Trim the excess length of the Trimlock to match the windshield.



Figure : Excess Trimlock




Figure : Properly Installed Trimlock

1. Place the windshield onto the machine. Make sure that the bottom edge of the windshield is flush with the plastic hood.

****

Figure : Positioned Windshield



Figure : Windshield Notch

1. Wrap the clamps onto the roll cage and align them with their corresponding windshield holes. Secure the windshield to the clamps using the 8 included Hex head machine screws and 8 flat washers.

****

Figure : Clamp Positioning

**Windshield Wiper Installation:**

1. Place the hardware onto the windshield wiper lever in the order indicated in Figures 7-10. If the machine already has a top, the lever must be adjusted so that it does not interfere with the top. Notice also how the interior requires an additional nut if a top is installed.

****

Figure : Interior Lever Hardware




Figure : Exterior Lever Hardware



Figure : Interior with Plastic Top



Figure : Exterior with Plastic Top

1. Tighten the exterior nut to slightly compress the plastic washer between the windshield and the exterior nut. Use a wrench to hold the lever shaft in place while tightening the exterior nut. Position the notches in the shaft vertically before installing the wiper.

****

Figure : Tightening Exterior Nut



Figure : Final Shaft Position

1. Remove the outermost nut from the windshield wiper shaft, position the wiper onto the shaft and then tighten the nut to secure the wiper to the assembly.

****

Figure : Wiper onto Shaft

1. Make sure that the wiper and lever align in a way that allows for convenient operation.

****

Figure : Final Alignment