**Safety:**

* Ensure that the UTV is safely parked on level ground with the ignition off.
* Wear all appropriate PPE for the following procedures.

**Note:**

* Leave all hardware loose until the entire assembly is in its final position.

**Assembly Components:**

Ensure that you have all of these components before beginning the installation.

**1 x Bumper**

**1 x Skid Plate**

**1 x Support Bracket**

**1 x Accent Plate**

**1 x Hardware Kit**

****

Figure : Kit Contents

**Installation:**

1. Remove the factory bumper.

****

Figure : Stock Bumper Removed

1. Attach the bumper support bracket to the machine using the 2 factory bolt holes indicated in Figure 2.


****

Figure : Bumper Support Bracket Mounted

1. Attach the skid plate to the bumper using the included 3/8” carriage bolts and nuts.

****

Figure : Skid Plate Mounted to Bumper

1. Attach the accent plate to the inside of the Bad Dawg logo using the included machine screws and nuts.

****

Figure : Accent Plate Behind Logo

1. Attach the skid plate to the bottom bolt holes located at the bottom of the machine.


****

Figure : Skid Plate Lower Mounting

1. Attach the face of the bumper to the bumper support bracket. At this point align the bumper with the factory bumper mounting location.

****

Figure : Skid Plate to Support Bracket


****

Figure : Stock Bumper Mounting Location

1. Attach the bumper to the factory mounting location using 3/8” bolts and nuts.


****

Figure : Bumper Mounting Bolt


****

Figure : Bumper Mounting Bolt Inside

1. Ensure that the bumper is properly aligned and straight before tightening all hardware securely.
2. Enjoy your ride!