**Safety:**

* Ensure that the UTV is safely parked on level ground with the ignition off.
* Wear all appropriate PPE for the following procedures.

**Note:**

* Leave all hardware loose until the entire assembly is in its final position.

**Assembly Components:**

Ensure that you have all of these components before beginning the installation.

**2 x CV Joint Protectors**

**2 x Mounting Brackets**

**1 x Hardware Kit**



Figure 1: Kit Contents

**Installation:**

**Note:** The following procedures show the installation performed on the front-passenger-side of the machine.

1. Remove the stock CV joint protector. Remove the two nuts and bolts holding the joint protector to the lower a-arm.




Figure 2: CV Joint Protector




Figure 3: Stock CV Joint Bolts

1. Match the correct metal CV joint protector mounting holes to the correct a-arm mounting location.



Figure 4: Joint Protector Mounting Location



Figure 5: Joint Protector Mounting Holes




Figure 6: Passenger Side Indicate

1. Position the new protector on the lower a-arm and insert the included hardware. Make sure that the carriage bolt is inserted into the square hole.



Figure : Mounting Bolts and Corresponding Nuts



Figure 8: Protector Mounted (Carriage Bolt Indicated)

1. Match the mounting bracket to the protector on the top side of the lower a-arm. Secure all of the bolts using the matching nuts. Make sure that the carriage bolt is secured with a washer and nylock nut.



Figure 9: Top Bracket (Carriage Bolt Indicated)

1. Repeat these procedures on the opposite side, ensuring that the hardware mirrors the passenger side setup.