**Safety:**

* Ensure that the UTV is safely parked on level ground with the ignition off.
* Wear all appropriate PPE for the following procedures.

**Note:**

* Leave all hardware loose until the entire assembly is in its final position.

**Assembly Components:**

Ensure that you have all of these components before beginning the installation.

**1 x Rear Bumper**

**1 x Hardware Kit**

**Installation:**

1. Remove the two factory bolts from the outside of the bottom of the cargo bed.

****

Figure : Exterior Mounting Point

1. Align the bumper with the mounting locations on the bed and frame under the center of the bed.

****

Figure : Positioned Bumper

****

Figure : Mounting Location Under the Bed

1. Utilize the factory bolts and supplied bolts and nuts to fasten the bumper to the machine.
2. Tighten all hardware securely.

****

Figure : Install Complete